Connection

1. Ensure that RaspberryPi and Laptop are connected to the same wifi network
2. Creds:
   1. IP: 10.136.18.55
   2. Username: pi
   3. Password: bassbot

Sending and receiving files:

1. On terminal, type:
2. Pi to Mac: scp pi@10.136.18.55:/home/pi/Desktop/BassBot/tuner.py . (‘dot’ with a space after source path means you’re saving it in the current directory.